| TUCSON(LM) >2010 > G 2.4 DOHC > Body Electrical System > Power Door Mirrors > Power Door Mirror Switch>Repair procedures |

Removal
Driver Door Mirror Switch
1. | Disconnect the negative battery terminal.
2. | Remove the front door trim. (Refer to the BD group - "Front door")
3. | Remove the screws from power window switch (A) and connectors (B).
4. | Remove the driver power window switch (A) from front door trim.
Be careful not to damage the hook when removing the switch module.
Installation
Driver Door Mirror Switch
1. | Install the driver power window switch and connectors.
2. | Install the front door trim.
Inspection
1. | Remove the front door trim and power door mirror switch module (A).
2. | Check for the continuity between terminals of power door mirror switch according to the table.