| TUCSON(LM) >2010 > G 2.4 DOHC > Clutch System > Clutch System > Clutch Master Cylinder>Repair procedures |

Removal
Do not spill brake fluid on the vehicle; it may damage the paint if brake fluid does contact the paint, wash it off immediately with water.
1. | Disconnect the push rod from the master cylinder by removing the snap pin (A) and washer (B).
2. | Disconnect the clutch tube (B) and reverse hose(A) from the clutch master cylinder.
3. | Remove the clutch master cylinder by turning it clockwise.(A)
Installation
1. | Installation is the reverse of removal.
• | Perform bleeding air procedure in concentric slave cylinder after pouring the brake fluid.(Refer to "Repair procedures" in CH group.)