| TUCSON(LM) >2010 > G 2.4 DOHC > Body (Interior and Exterior) > Seat Belt > Front Seat Belt>Repair procedures |

Replacement
Front Seat Belt Replacement
• | When installing the belt, make sure not to damaged the pretensioner.
1. | Remove the following items first :
A. | Front door scuff trim (Refer to the BD group - "Interior Trim")
B. | Rear door scuff trim (Refer to the BD group - "Interior Trim")
2. | After raise the lower anchor cover (A), loosen the lower anchor (B) mounting bolt.
Tightening torque : 39.2 ~ 53.9 N.m (4.0 ~ 5.5 kgf.m, 28.9 ~ 39.8 lb-ft)
3. | Remove the center lower pillar trim (A).
4. | Remove the cap.
5. | After loosening the mounting bolt, then remove the center upper pillar trim (A) .
6. | After loosening the mounting bolt, then remove the upper anchor (A).
Tightening torque : 39.2 ~ 53.9 N.m (4.0 ~ 5.5 kgf.m, 28.9 ~ 39.8 lb-ft)
7. | After disconnecting the pretensioner connector lock pin, remove the pretensioner connector (B), loosen the mounting bolt, then remove the pretensioner (A).
Tightening torque : 39.2 ~ 53.9 N.m (4.0 ~ 5.5 kgf.m, 28.9 ~ 39.8 lb-ft)
8. | Installation is the reverse of removal.
Height Adjust Relacement
1. | Remove the following items first :
A. | Front door scuff trim (Refer to the BD group - "Interior Trim")
B. | Rear door scuff trim (Refer to the BD group - "Interior Trim")
C. | Front seat belt lower anchor
D. | Front seat belt upper anchor
E. | Center lower pillar trim (Refer to the BD group - "Interior Trim")
F. | Center upper fillar trim (Refer to the BD group - "Interior Trim")
2. | After loosening the mounting bolt, then remove the hight adjustor (A).
Tightening torque : 39.2 ~ 53.9 N.m (4.0 ~ 5.5 kgf.m, 28.9 ~ 39.8 lb-ft)
3. | Installation is the reverse of removal.
• | Replace ant damaged clips.
• | Make sure the height adjust properly.
Front Seat Belt Buckle Relacement
1. | Remove the front seat. (Refer to the BD group - "Front Seat")
2. | After loosening the mounting bolt, then remove the front seat belt buckle (A).
Tightening torque : 39.2 ~ 53.9 N.m (4.0 ~ 5.5 kgf.m, 28.9 ~ 39.8 lb-ft)
3. | Installation is the reverse of removal.