| TUCSON(LM) >2010 > G 2.4 DOHC > Body Electrical System > Keyless Entry And Burglar Alarm > Transmitter>Specifications |

Specifications
Item | Specification
Rated voltage | DC 3V
Temperature range | -4°F ~ 140°F (-20°C ~ +60°C)
RF Modulation method | FSK
Keyless entry transmitterPower source | Lithium 3V battery (1EA)
Transmissible distance | 30m or more
Life of battery | 2 years or more (at 20 times per day)
Button | 3 (Door lock, Door unlock, Tailgate)
Transmission frequency | 313.85 MHz