| TUCSON(LM) >2010 > G 2.4 DOHC > Engine Mechanical System > Lubrication System > Oil Pressure Switch>Repair procedures |

Inspection
1. | Check the continuity between the terminal and the body with an ohmmeter. If there is no continuity, replace the oil pressure switch.
2. | Check the continuity between the terminal and the body when the fine wire is pushed. If there is continuity even when the fine wire is pushed, replace the switch.
3. | If there is no continuity when a 50kpa (7psi) is applied throgh the oil hole, the switch is operaing properly. Check for air leakage. If air leaks, the diaphragm is broken. Replace it.