| TUCSON(LM) >2011 > G 2.0 DOHC > Body Electrical System > Smart key System > Smart key unit>Repair procedures |

Removal
Smart Key Unit
1. | Disconnect the negative (-) battery terminal.
2. | Remove the glove box housing. (Refer to the BD group - "Crash pad")
3. | After disconnecting the smart key unit connector (A), loosen the smart key unit mounting bolts, and remove the smart key unit (B).
RF Receiver
1. | Disconnect the negative (-) battery terminal.
2. | Remove the glove box housing. (Refer to the BD group - "Crash pad")
3. | Remove the air vent housing in front of the assist seat. (Refer to the BD group - "Crach pad")
4. | After loosening the mounting nut (B), disconnect the connector (A) and remove the receiver (C).
Interior 1 Antenna
1. | Disconnect the negative (-) battery terminal.
2. | Remove the seat heater switch assembly. (Refer to the BE group - "Seat heater")
3. | After loosening the antenna nuts (2EA) and connector (B), remove the interior 1 antenna (A).
Release the connector lock (A) as indicated by the arrow, and then push-down the lock. Make sure the connector is locked completely when installing.
Interior 2 Antenna
1. | Disconnect the negative (-) battery terminal.
2. | Remove the floor console rear panel (A) using the appropriate tool.
Take care not to damage and scratch the floor console rear panel and its related parts. Take care not to damage the hook when removing the floor console rear panel.
3. | After loosening the antenna nuts (2EA) and connector, remove the interior 2 antenna (A).
Release the connector lock (A) as indicated by the arrow, and then push-down the lock. Make sure the connector is locked completely when installing.
Interior 3 Antenna
1. | Disconnect the negative (-) battery terminal.
2. | After loosening the mounting bolts, then remove the rear seat assembly. (Refer to the BD group - "Rear seat")
3. | After loosening the antenna nuts (2EA) and connector (A), remove the interior 3 antenna (B).
Release the connector lock (A) as indicated by the arrow, and then push-down the lock. Make sure the connector is locked completely when installing.
Exterior Bumper Antenna
1. | Disconnect the negative (-) battery terminal.
2. | Lift the vehicle up using the lift. (Refer to the GI group - "Lift And Support Points")
3. | Disconnect the antenna connector (A) on the center of rear bumper.
4. | After loosening the nuts (2EA), remove the exterior bumper antenna (B).
Buzzer
1. | Disconnect the negative (-) battery terminal.
2. | Remove the front left fender. (Refer to the BD group - "Fender")
3. | Disconnect the connectors, then remove the buzzer (A).
Door Outside Handle
1. | Disconnect the negative (-) battery terminal.
2. | Disconnect the connector after removing the door trim. (Refer to the BD group - "Front door")
3. | After loosening the mounting bolt, then remove the key holder (A).
4. | Remove the outside handle (A) by sliding it rearward.
5. | Disconnect the outside handle connector (B).
Tailgate Switch
1. | Disconnect the negative (-) battery terminal.
2. | Remove the tailgate trim. (Refer to the BD group - "Tailgate trim")
3. | Disconnect the connector. After loosening the tailgate garnish mounting nuts (13EA), remove the tailgate garnish (A).
4. | Remove the outside handle (A) after loosening the outside handle mounting screws.
5. | Remove the other wiring connectors which connected with outside handle, then remove the tailgate switch assembly (A).
Inspection
Smart Key Unit
- | Refer to BE group - inspection / self diagnosis with scan tool.
Smart Key Switch
- | Refer to BE group - inspection / self diagnosis with scan tool.
Antenna
- | Refer to BE group - inspection / self diagnosis with scan tool.
Tailgate Switch
1. | Check for continuity between the tailgate latch terminals.
2. | If continuity is not specified, inspect the switch
Installation
Smart Key Unit
1. | Install the smart key unit.
2. | Install the smart key unit mounting bolt and nut, and then connect the connector.
3. | Install the glove box.
4. | Install the negative (-) battery terminal and check the smart key system.
RF Receiver
1. | Install the RF receiver.
2. | Install the glove box housing and air vent housing.
3. | Install the negative (-) battery terminal and check the smart key system.
Interior 1 Antenna
1. | Install the interior 1 antenna.
2. | Install the front seat heater switch assembly.
3. | Install the negative (-) battery terminal and check the smart key system.
Interior 2 Antenna
1. | Install the interior 2 antenna.
2. | Install the floor console rear cover after connecting the connector.
3. | Install the negative (-) battery terminal and check the smart key system.
Interior 3 Antenna
1. | Install the interior 3 antenna.
2. | Install the rear seat assembly.
3. | Install the negative (-) battery terminal and check the smart key system.
Exterior Bumper Antenna
1. | Install the exterior bumper antenna.
2. | Install the negative (-) battery terminal and check the smart key system.
Buzzer
1. | Install the buzzer.
2. | Install the front left fender.
3. | Install the negative (-) battery terminal and check the smart key system.
Door Outside Handle
1. | Install the outside handle.
2. | Install the door trim.
3. | Install the negative (-) battery terminal and check the smart key system.
Tailgate Switch
1. | Install the tailgate switch.
2. | Install the tailgate garnish.
3. | Install the tailgate trim.
4. | Install the negative (-) battery terminal and check the smart key system.