| TUCSON(LM) >2011 > G 2.0 DOHC > Body (Interior and Exterior) > Interior > Console>Repair procedures |

Replacement
Console Assembly Replacement
• | When prying with a flat-up screwdriver, wrap it with protective tape, and apply protective tape around the related parts, to prevent damage.
• | Put on gloves to protect your hands.
1. | Remove the knob (A).
2. | Using a screwdriver, remove the floor console tray (A).
3. | Using a screwdriver, remove the floor console bezel (A).
4. | Disconnect the connectors (B).
5. | Using a screwdriver, remove the console upper cover (A).
6. | Disconnect the connector (B).
7. | Remove the console tray mat (A).
8. | Remove the extension side cover (A).
9. | After loosening the mounting bolts and screws, then remove the floor console assembly (A).
10. | Installation is the reverse of removal.
• | Make sure the connector is plugged in properly.
• | Replace any damage clips.