| TUCSON(LM) >2011 > G 2.0 DOHC > Body Electrical System > Seat Electrical > Power Seat Control Switch>Repair procedures |

Inspection
1. | With the power seat switch in each position, make sure that continuity exists between the terminals below. If continuity is not as specified, replace the power seat switch.
Removal
1. | Disconnect the negative (-) battery terminal.
2. | Remove the power seat recliner cover. (Refer to the BD group - "Front seat")
3. | Remove the power seat control switch (A).
Installation
1. | Install the power seat control switch after connecting the connector.
2. | Install the recliner cover and front power seat.