| TUCSON(LM) >2011 > G 2.0 DOHC > Engine Mechanical System > Cooling System > Coolant>Repair procedures |

Replacement And Air Bleeding
Never remove the radiator cap when the engine is hot. Serious scalding could be caused by hot fluid under high pressure escaping from the radiator.
When pouring engine coolant, be sure to shut the relay box lid and not to let coolant spill on the electrical parts or the paint. If any coolant spills, rinse it off immediately.
1. | Make sure the engine and radiator are cool to the touch.
2. | Remove radiator cap.
3. | Loosen the drain plug, and drain the coolant
4. | Tighten the radiator drain plug securely.
5. | After draining engine coolant in the reservoir tank, clean the tank.
6. | Fill the radiator with water through the radiator cap and tighten the cap.
Pressure can blow water back out the radiator cap-pour water slowly while intermittently squeezing the radiator hoses.
7. | After warming up the engine until the cooling fan operates several times, accelerate it at idle.
8. | Wait until the engine is cool.
9. | Repeat the step 1 to 8 until the drained water is clean.
10. | Fill fluid mixture with coolant and water(5 : 5) (Tropical region – 4:6) slowly through the radiator cap. Push the upper/lower hoses of the radiator so as bleed air easily.
• | Use only genuine antifreeze/coolant.
• | For best corrosion protection, the coolant concentration must be maintained year-round at 35% minimum. Coolant concentrations less than 35% may not provide sufficient protection against corrosion or freezing.
• | Coolant concentrations greater then 60% will impair cooling efficiency and are not recommended.
• | Do not mix different brands of antifreeze/coolants.
• | Do not use additional rust inhibitors or antirust products; they may not be compatible with the coolant.
11. | Start the engine and run coolant circulates. When the cooling fan operates and coolant circulates, refill coolant through the radiator cap.
12. | Repeat 11 until the cooling fan 3 ~ 5times and bleed air sufficiently out of the cooling system.
13. | Install the radiator cap and fill the reservoir tank to the "MAX" line with coolant.
14. | Run the vehicle under idle until the cooling fan operates 2 ~ 3 times.
15. | Stop the engine and wait coolant to cool.
16. | Repeat step.10 to step.15 until the coolant level doesn't fall any more, bleed air out of the cooling system
As it is to bleed air out to the cooling system and refill coolant when coolant gets cool completely, recheck the coolant level in the reservoir tank for 2 ~ 3 days after replacing coolant.
Coolant capacity : 6.8L (7.2US qt, 5.9lmp qt)