| TUCSON(LM) >2011 > G 2.0 DOHC > Restraint > Seat Belt Pretensioner > Anchor Pretensioner>Repair procedures |

Removal
1. | Disconnect the battery negative cable, and wait for at least three minutes before beginning work.
2. | To remove the seat belt anchor pretensioner (C), keep on pushing the lock pins (A) as arrow direction. And then remove the seat belt after pushing the lock pin (B).
3. | Remove the following parts. (Refer to the Body group-Interior trim)
A. | Door scuff trim
B. | Center pillar trim
4. | Disconnect the anchor pretensioner connector (A).
5. | Loosen the anchor pretensioner mounting bolt (B) and remove the anchor pretensioner.
Installation
1. | Remove ignition key from the vehicle.
2. | Disconnect the negative (-) cable from battery and wait for at least three minutes.
3. | Install the anchor pretensioner with a bolt.
Tightening torque: 39.2 ~ 53.9 N.m (4.0 ~ 5.5 kgf.m, 28.9 ~ 39.8 lb-ft)
4. | Connect the anchor pretensioner connector.
5. | Install the following parts. (Refer to the body group - Interior trim)
A. | Center pillar trim
B. | Door scuff trim
6. | Insert the seat belt to the anchor pretensioner.
Make sure the lock pin is connected in properly.
7. | Reconnect the battery negative cable.
8. | After installing the anchor pretensioner, confirm proper system operation:
A. | Turn the ignition switch ON; the SRS indicator light should be turned on for about six seconds and then go off.