| TUCSON(LM) >2011 > G 2.0 DOHC > Emission Control System > Evaporative Emission Control System > Fuel Tank Air Filter>Repair procedures |

Removal
1. | Turn the ignition switch OFF and disconnect the battery negative (-) cable.
2. | Lift the vehicle with a jack.
3. | Disconnect the canister close valve connector (A).
4. | Disconnect the ventilation hose (B) and vapor hose (C).
5. | Remove the fuel tank air filter and canister close valve assembly (A) after removing the installation nut (B).
6. | Release the lever (A), and then separate the canister close valve (B) from the fuel tank air filter (C) after rotating it in the direction of the arrow in the figure.
7. | Install a new fuel tank air filter in accordance with the reverse order.