| TUCSON(LM) >2011 > G 2.0 DOHC > Fuel System > Engine Control System > Fuel Tank Pressure Sensor (FTPS)>Repair procedures |

Inspection
1. | Connect the GDS on the Data Link Connector (DLC).
2. | Measure the output voltage of the FTPS.
Specification: Refer to "Specification"
Removal
1. | Turn the ignition switch OFF and disconnect the battery negative (-) cable.
2. | Remove the rear seat (Refer to "Seat" in BD group).
3. | Remove the fuel pump service cover (A).
4. | Disconnect the fuel tank pressure sensor connector (A).
5. | Remove the fuel tank pressure sensor after releasing the hooks vertically.
Installation
• | Install the component with the specified torques.
• | Note that internal damage may occur when the component is dropped. In this case, use it after inspecting.
• | Insert the sensor in the installation hole and be careful not to damage when installation.
1. | Installation is reverse of removal.