| TUCSON(LM) >2011 > G 2.0 DOHC > Body Electrical System > Power Door Mirrors > Power Door Mirror Actuator>Repair procedures |

Inspection
1. | Disconnect the negative (-) battery terminal.
2. | Remove the front door delta cover. (Refer to the BD group - "Front door")
3. | Disconnect the connector from the door mirror.
4. | Verify that the mirror operates properly as shown in the table. Mirror Heater Turn Signal Lamp