| TUCSON(LM) >2011 > G 2.0 DOHC > Heating,Ventilation, Air Conditioning > Controller > Heater & A/C Control Unit(Manual)>Repair procedures |

Replacement
1. | Disconnect the negative (-) battery terminal.
2. | Remove the console upper cover (A).
3. | Using the screwdriver, remove the center facia lower cover (A).
4. | Using the screwdriver, remove the center facia lower switch assembly (A).
5. | Disconnect the connectors and then remove the center facia lower switch assembly (A).
6. | Loosen the control panel mounting screws and then remove the control panel (A).
7. | Disconnect the connectors and then remove the control panel (A).
8. | Installation is the reverse order of removal.