| TUCSON(LM) >2011 > G 2.0 DOHC > Body Electrical System > Fuses And Relays > ICM (Integrated Circuit Module) Relay Box>Repair procedures |

Inspection
Rear Wiper Relay Check for continuity between the terminals.
1. | There should be continuity between the No.11 in the A and No.12 in the A terminals when power and ground are connected to the No.2 in the A and No.11 in the A terminals.
2. | There should be no continuity between the No.11 in the A and No.12 in the A terminals when power is disconnected.
Flasher Sound Relay Check for continuity between the terminals.
1. | There should be continuity between the No.4 in the B and No.6 in the B terminals when power and ground are connected to the No.4 in the B and No.5 in the B terminals.
2. | There should be no continuity between the No.4 in the B and No.6 in the B terminals in the A terminals when power is disconnected.
DBC Relay Check for continuity between the terminals.
1. | There should be continuity between the No.3 in the A and No.8 in the A terminals when power and ground are connected to the No.5 in the A and No.6 in the A terminals.
2. | There should be no continuity between the No.3 in the A and No.8 in the A terminals when power is disconnected.
Two Turn Unlock Relay Check for continuity between the terminals.
1. | There should be continuity between the No.17 in the A and No.18 in the A terminals when power and ground are connected to the No.16 in the A and No.17 in the A terminals.
2. | There should be continuity between the No.15 in the A and No.18 in the A terminals when power is disconnected.