| TUCSON(LM) >2011 > G 2.0 DOHC > Fuel System > Engine Control System > Variable Intake Solenoid (VIS) Valve>Repair procedures |

Inspection
1. | Turn the ignition switch OFF.
2. | Disconnect the VIS valve connector.
3. | Measure resistance between VIS valve terminals 1 and 2.
Specification: Refer to "Specification"
Removal
1. | Turn the ignition switch OFF and disconnect the battery negative (-) cable.
2. | Disconnect the variable intake solenoid valve connector (A).
3. | Disconnect the vacuum hoses (B) from the valve.
4. | Remove the installation nut (C), and then remove the valve from the surge tank.
Installation
• | Install the component with the specified torques.
• | Note that internal damage may occur when the component is dropped. In this case, use it after inspecting.
• | Be careful of foreign material not to flow into the valve.
1. | Installation is reverse of removal.