| TUCSON(LM) >2011 > G 2.0 DOHC > Fuel System > General Information>Specifications |

Specifications
Fuel Delivery System
Items | Specification
Fuel Tank | Capacity | 55 lit. (14.5 U.S.gal., 58.1 U.S.qt., 48.3 Imp.qt.)
Fuel Filter | Type | Paper type
Fuel Pressure Regulator | Regulated Fuel Pressure | 324 ~ 363 kPa (3.3 ~ 3.7 kgf/cm², 46.9 ~ 52.6 psi)
Fuel Pump | Type | Electrical, in-tank type
Driven by | Electric motor
Sensors
Manifold Absolute Pressure Sensor (MAPS) ▷ Type: Piezo-resistive pressure sensor type ▷ Specification
Pressure [kPa (kgf/cm², psi)] | Output Voltage (V)
20.0 (0.20, 2.9) | 0.79
46.7 (0.47, 6.77) | 1.84
101.3 (1.03, 14.7) | 4.0
Intake Air Temperature Sensor (IATS) ▷ Type: Thermistor type ▷ Specification
Temperature [°C(°F)] | Resistance (kΩ)
-40(-40) | 40.93 ~ 48.35
-20(-4) | 13.89 ~ 16.03
0(32) | 5.38 ~ 6.09
10(50) | 3.48 ~ 3.90
20(68) | 2.31 ~ 2.57
40(104) | 1.08 ~ 1.21
50(122) | 0.76 ~ 0.85
60(140) | 0.54 ~ 0.62
80(176) | 0.29 ~ 0.34
Engine Coolant Temperature Sensor (ECTS) ▷ Type: Thermistor type ▷ Specification
Temperature [°C(°F)] | Resistance (kΩ)
-40(-40) | 48.14
-20(-4) | 14.13 ~ 16.83
0(32) | 5.79
20(68) | 2.31 ~ 2.59
40(104) | 1.15
60(140) | 0.59
80(176) | 0.32
Throttle Position Sensor (TPS) [integrated into ETC Module] ▷ Type: Variable resistor type ▷ Specification
Throttle Angle(°) | Output Voltage (V)
TPS1 | TPS2
0 | 0 | 5.0
10 | 0.48 | 4.52
20 | 0.95 | 4.05
30 | 1.43 | 3.57
40 | 1.90 | 3.10
50 | 2.38 | 2.62
60 | 2.86 | 2.14
70 | 3.33 | 1.67
80 | 3.81 | 1.19
90 | 4.29 | 0.71
100 | 4.76 | 0.24
105 | 5.0 | 0
C.T (6~15°) | 0.29 ~ 0.71 | 4.29 ~ 4.71
W.O.T (93~102°) | 4.43 ~ 4.86 | 0.14 ~ 0.57
Item | Resistance (kΩ)
TPS1 | 0.875 ~ 1.625 [20°C(68°F)]
TPS2 | 0.875 ~ 1.625 [20°C(68°F)]
Crankshaft Position Sensor (CKPS) ▷ Type: Hall effect type Camshaft Position Sensor (CMPS) ▷ Type: Hall effect type Knock Sensor (KS) ▷ Type: Piezo-electricity type ▷ Specification
Item | Specification
Capacitance (pF) | 850 ~ 1,150
Heated Oxygen Sensor (HO2S) [Bank 1/Sensor 1] ▷ Type: Zirconia (ZrO2) [Linear] type ▷ Specification
Item | Specification
Heater Resistance (Ω) | 2.5 ~ 4.0 [20°C(69.8°F)]
Heated Oxygen Sensor (HO2S) [Bank 1/Sensor 2] ▷ Type: Zirconia (ZrO2) [Binary] type ▷ Specification
A/F Ratio (λ) | Output Voltage(V)
RICH | Approx. 0.9
LEAN | Approx. 0.04
Item | Specification
Heater Resistance (Ω) | 3.3 ~ 4.1 [21°C(69.8°F)]
Accelerator Position Sensor (APS) ▷ Type: Variable resistor type ▷ Specification
Accelerator Position | Output Voltage (V)
APS1 | APS2
C.T | 0.7 ~ 0.8 | 0.29 ~ 0.46
W.O.T | 3.85 ~ 4.35 | 1.93 ~ 2.18
Fuel Tank Pressure Sensor (FTPS) ▷ Type: Piezo - Resistivity type ▷ Specification
Pressure [kPa (kgf/cm², in H2O) | Output Voltage (V)
-6.67 (-0.068, -26.8) | 0.5
0 | 2.5
+6.67 (0.068, 26.8) | 4.5
Actuators
Injector ▷ Specification
Item | Specification
Coil Resistance (Ω) | 13.8 ~ 15.2 [20°C(68°F)]
ETC Motor [integrated into ETC Module] ▷ Specification
Item | Specification
Coil Resistance (Ω) | 1.2 ~ 1.8 [20°C(68°F)]
Purge Control Solenoid Valve (PCSV) ▷ Specification
Item | Specification
Coil Resistance (Ω) | 19.0 ~ 22.0 [20°C(68°F)]
CVVT Oil Control Valve (OCV) ▷ Specification
Item | Specification
Coil Resistance (Ω) | 6.9 ~ 7.9 [20°C(68°F)]
Variable Intake Solenoid (VIS) Valve ▷ Specification
Item | Specification
Coil Resistance (Ω) | 30.0 ~ 35.0 [20°C(68°F)]
Variable Charge Motion Actuator (VCMA) ▷ Specification [Motor]
Item | Specification
Coil Resistance (Ω) | 3.4 ~ 4.4 [20°C(68°F)]
[Position Sensor]
Item | Specification
Coil Resistance (kΩ) | 3.44 ~ 5.16 [20°C(68°F)]
Ignition Coil ▷ Type: Stick type ▷ Specification
Item | Specification
Primary Coil Resistance (Ω) | 0.62 ± 10％[20°C(68°F)]
Secondary Coil Resistance (kΩ) | 7.0 ± 15％[20°C(68°F)]
Canister Close Valve (CCV) ▷ Specification
Item | Specification
Coil Resistance (Ω) | 19.8 ~ 21.8 [20°C(68°F)]
Service Standard
Item | Specification
Ignition Timing (°) | BTDC 8 ± 10
Idle Speed (rpm) | A/C OFF | Neutral, N, P-range | 620 ± 100
D-range | 620 ± 100
A/C ON | Neutral, N, P-range | 620 ± 100
D-range | 620 ± 100
Tightening Torques
Engine Control System
Item | kgf.m | N.m | lb-ft
ECM installation bolt | 0.8 ~ 1.2 | 7.8 ~ 11.8 | 5.8 ~ 8.7
Manifold absolute pressure sensor installation bolt | 1.0 ~ 1.2 | 9.8 ~ 11.8 | 7.2 ~ 8.7
Crankshaft position sensor installation bolt | 1.0 ~ 1.2 | 9.8 ~ 11.8 | 7.2 ~ 8.7
Crankshaft position sensor cover installation bolt (M8) | 1.9 ~ 2.4 | 18.6 ~ 23.5 | 13.7 ~ 17.4
Crankshaft position sensor cover installation bolt (M6) | 1.0 ~ 1.2 | 9.8 ~ 11.8 | 7.2 ~ 8.7
Camshaft position sensor (Bank 1 / Intake) installation bolt | 1.0 ~ 1.2 | 9.8 ~ 11.8 | 7.2 ~ 8.7
Camshaft position sensor (Bank 1 / Exhaust) installation bolt | 1.0 ~ 1.2 | 9.8 ~ 11.8 | 7.2 ~ 8.7
Knock sensor installation bolt | 1.9 ~ 2.4 | 18.6 ~ 23.5 | 13.7 ~ 17.4
Heated oxygen sensor (Bank 1 / sensor 1) installation [SULEV] | 4.0 ~ 5.0 | 39.2 ~ 49.1 | 28.9 ~ 36.2
Heated oxygen sensor (Bank 1 / sensor 2) installation [SULEV] | 4.0 ~ 5.0 | 39.2 ~ 49.1 | 28.9 ~ 36.2
Heated oxygen sensor (Bank 1 / sensor 1) installation [ULEV] | 4.5 ~ 5.0 | 44.1 ~ 49.1 | 32.6 ~ 36.2
Heated oxygen sensor (Bank 1 / sensor 2) installation [ULEV] | 4.5 ~ 5.0 | 44.1 ~ 49.1 | 32.6 ~ 36.2
Electronic throttle body installation bolt | 0.8 ~ 1.2 | 7.8 ~ 11.8 | 5.8 ~ 8.7
Purge control solenoid valve bracket installation bolt | 1.0 ~ 1.2 | 9.8 ~ 11.8 | 7.2 ~ 8.7
CVVT oil control valve (Bank 1 / Intake) installation bolt | 1.0 ~ 1.2 | 9.8 ~ 11.8 | 7.2 ~ 8.7
CVVT oil control valve (Bank 1 / Exhaust) installation bolt | 1.0 ~ 1.2 | 9.8 ~ 11.8 | 7.2 ~ 8.7
Ignition coil installation bolt | 1.0 ~ 1.2 | 9.8 ~ 11.8 | 7.2 ~ 8.7
Canister close valve & fuel tank air filter bracket installation nut | 0.8 ~ 1.2 | 7.8 ~ 11.8 | 5.8 ~ 8.7
Variable charge motion actuator installation bolt | 0.8 ~ 1.2 | 7.8 ~ 11.8 | 5.8 ~ 8.7
Fuel Delivery System
Item | kgf.m | N.m | lb-ft
Fuel tank installation nut | 4.0 ~ 5.5 | 39.2 ~ 54.0 | 28.9 ~ 39.8
Filler-neck assembly bracket installation nut | 0.4 ~ 0.6 | 3.9 ~ 5.9 | 2.9 ~ 4.3
Accelerator pedal module installation nut | 1.7 ~ 2.6 | 16.7 ~ 25.5 | 12.3 ~ 18.8
Accelerator pedal module installation bolt | 0.8 ~ 1.2 | 7.8 ~ 11.8 | 5.8 ~ 8.7
Delivery pipe installation bolt | 1.9 ~ 2.4 | 18.6 ~ 23.5 | 13.7 ~ 17.4
Delivery pipe installation nut (↔ Fuel feed tube) | 0.8 ~ 1.0 | 7.8 ~ 9.8 | 5.8 ~ 7.2
Fuel pump locking ring (Loosening torque) | Min. 7 | Min. 68.65 | Min. 50.6