| TUCSON(LM) >2011 > G 2.4 DOHC > Suspension System > Rear Suspension System > Rear Stabilizer Bar>Repair procedures |

Replacement
1. | Remove the rear wheel & tire.
Tightening torque : 88.3 ~ 107.9N.m(9.0 ~ 11.0Kgf.m, 65.1 ~ 79.6lb-ft)
Be careful not to damage to the hub bolts when removing the front wheel & tire.
2. | Loosen the nut and then remove the rear stabilizer link(B) with the rear lower arm(A).
Tightening torque : 98.1 ~ 117.7N.m(10.0 ~ 12.0Kgf.m, 72.3 ~ 86.8lb-ft)
3. | Loosen the mounting bolt and then remove the stabilizer bar(A) with the sub frame.
Tightening torque : 44.1 ~ 53.9N.m(4.5 ~ 5.5Kgf.m, 32.5 ~ 39.8lb-ft)
4. | Installation is the reverse of removal.
Inspection
1. | Check the rear stabilizer bar for deformation.
2. | Check the rear stabilizer link ball joint for damage.