| TUCSON(LM) >2011 > G 2.4 DOHC > Body Electrical System > Windshield Deicer > Windshield Deicer>Repair procedures |

Inspection
1. | Remove the cowl top cover. (Refer to the wiper)
2. | Disconnect the windshield deicer connector (A) from the wiper motor linkage.
3. | Check for continuity between the terminals of deicer lines.
4. | Turn the ignition switch ON and the windshield deicer switch ON, then measure the voltage between the terminals of harness side deicer connector.
OK : approx. Battery voltage