| TUCSON(LM) >2011 > G 2.4 DOHC > Fuel System > Engine Control System > Purge Control Solenoid Valve (PCSV)>Repair procedures |

Inspection
1. | Turn the ignition switch OFF.
2. | Disconnect the PCSV connector.
3. | Measure resistance between the PCSV terminals 1 and 2.
4. | Check that the resistance is within the specification.
Specification: Refer to “Specification”
Removal
1. | Turn the ignition switch OFF and disconnect the battery negative (-) cable.
2. | Disconnect the purge control solenoid valve connector (A).
3. | Disconnect the vapor hoses (B) from the purge control solenoid valve.
4. | Remove the bracket installation bolt (C), and then remove the valve from the surge tank.
Installation
• | Install the component with the specified torques.
• | Note that internal damage may occur when the component is dropped. In this case, use it after inspecting.
• | Use care to keep foreign material out of the valve.
1. | Installation is reverse of removal.
Purge control solenoid valve bracket installation bolt: 9.8 ~ 11.8 N.m (1.0 ~ 1.2 kgf.m, 7.2 ~ 8.7 lb-ft)