| TUCSON(LM) >2011 > G 2.4 DOHC > Body (Interior and Exterior) > Bumper > Front Bumper>Repair procedures |

Replacement
• | Put on gloves to protect your hands.
• | When prying with a flat-tip screwdriver, wrap it with protective tape to prevent damage.
• | Take care not bend or scratch the cover and other parts.
1. | Loosen the radiator upper cover mounting bolts and clips.
2. | Remove the mounting clips.
3. | After loosening the front bumper side’s mounting screw and clip, then disconnect the side’s.
4. | Push the lock pin, disconnect the fog lamp connector (A).
5. | Remove the front bumper.
6. | Installation is the reverse of removal.
• | Make sure the connector is plugged in properly.
• | Replace any damage clips.