| TUCSON(LM) >2011 > G 2.4 DOHC > Fuel System > Fuel Delivery System > Accelerator Pedal>Repair procedures |

Removal
1. | Turn the ignition switch OFF and disconnect the negative (-) battery cable.
2. | Disconnect the accelerator position sensor connector (A).
3. | Remove the installation nuts (B), the bolt (C) and then remove the accelerator pedal module.
Installation
1. | Installation is reverse of removal.
Accelerator pedal module installation nut: 16.7 ~ 25.5 N.m (1.7 ~ 2.6 kgf.m, 12.3 ~ 18.8 lb-ft) Accelerator pedal module installation bolt: 7.8 ~ 11.8 N.m (0.8 ~ 1.2 kgf.m, 5.8 ~ 8.7 lb-ft)