| TUCSON(LM) >2011 > G 2.4 DOHC > Body Electrical System > Lighting System > Overhead Console Lamp>Repair procedures |

Inspection
Remove the overhead console lamp assembly then check for continuity between terminals. If the continuity is not as specified, replace the map lamp switch.
Removal
1. | Disconnect the negative (-) battery terminal.
2. | Remove the overhead console lamp assembly. (Refer to the BD group - "Roof trim")
3. | Remove the overhead console bulb (B) after disconnecting the panoramaroof switch connector and lamp connector (A).
4. | When replacing the bulb only, release the lens (C) cover from the roof without removing the overhead console lamp assembly.
Installation
1. | Install the bulbs and connect the connectors.
2. | Install the overhead console lamp assembly.