| TUCSON(LM) >2011 > G 2.4 DOHC > Body (Interior and Exterior) > Exterior > Mirror>Repair procedures |

Replacement
Outside Rear View Mirror Assembly Replacement
• | When prying with a flat-up screwdriver, wrap it with protective tape, and apply protective tape around the related parts, to prevent damage.
• | Put on gloves to protect your hands.
1. | Using a screwdriver, remove the quadrant inner cover (A).
2. | After disconnecting the connector (A), then remove the outside rear view mirror (B).
Tightening torque : 6.9 ~ 10.8 N.m (0.7 ~ 1.1 kgf.m, 5.1 ~ 8.0 lb-ft)
3. | Installation is the reverse of removal.
Inside Rear View Mirror Assembly Replacement
Mirror Replacement
1. | Push the inside rear view mirror base (A) down to remove the inside rear view mirror assembly (B).
2. | Installation is the reverse of removal.
ECM Mirror Replacement
1. | Using a screwdriver, remove the ECM mirror cover (A).
2. | Disconnect the connector (A).
3. | Loosen the mounting screw (C), push the ECM mirror base UP to remove the ECM mirror assembly (B).
4. | Installation is the reverse of removal.