| TUCSON(LM) >2011 > G 2.4 DOHC > Restraint > SRSCM > Seat Belt Buckle Switch (BS)>Repair procedures |

Removal
1. | Disconnect the battery negative cable, and wait for at least three minutes before beginning work.
2. | Remove the front seat assembly. (Refer to the Body group- Front seat)
3. | Loosen the seat belt buckle mounting bolt and remove the seat belt buckle switch.
Installation
Be sure to install the harness wires not to be pinched or interfered with other parts.
1. | Remove the ignition key from the vehicle.
2. | Disconnect the battery negative cable, and wait for at least three minutes before beginning work.
3. | Install the seat belt buckle switch.
Tightening Torque: 39.2 ~ 53.9 N.m (4.0 ~ 5.5 kgf.m, 28.9 ~ 39.8 lb-ft)
4. | Install the front seat assembly. (Refer to the Body group - Front seat)
5. | Reconnect the battery negative cable.
6. | After installing the seat belt buckle switch, confirm proper system operation:
A. | Turn the ignition switch ON; the SRS indicator should be turned on for about six seconds and then go off.