| TUCSON(LM) >2011 > G 2.4 DOHC > Body (Interior and Exterior) > Seat & Power Seat > Rear Seat>Repair procedures |

Replacement
Seat Assembly Replacement
1. | After loosening the mounting bolts, then remove the rear seat back assembly (A).
Tightening torque : 44.1 ~ 58.8 N.m (4.5 ~ 6.0 kgf.m, 32.5 ~ 43.4 lb-ft)
2. | Disconnect the connector (A), then remove the rear seat cushion assembly.
3. | Installation is the reverse of removal.
Seat mounting bolt and nut installation procedure.
• | Tighten temporarily in the order of nut and bolt on the front of recliner hinge installation part.
• | After completely tightening completely the bolt on the back of the recliner hinge installaion part, tighten the bolt on the front of it completely.
• | Setting down the seat cushion, tighten the mounting bolt of the cushion frame hinge.
• | Check if reclining the seat and folding seat back operate smoothly.
Seat Back Cover Replacement [RH]
1. | Push the lock pin (B), and then remove the headrest (A).
2. | After loosening the mounting screw, then remove the rear bag hook (A).
3. | Using a screwdriver or remover, remove the tether anchor garnish (B).
4. | Using a long nose, remove the rock pin (B) and armrest (A).
5. | Using a screwdriver or remover, remove the upper bezel (A).
6. | Zip off the seat back cover (A), and then full it up.
7. | Remove the hogring clips (A) and screw.
8. | Disonnect the hook (B).
9. | Pull out the headrest guides (A) while pinching the end of the guides, and remove them.
10. | Disconnect the seat back cover (A) from the seat back frame (B).
11. | Disconnect the hogring clips (B) on the front of seat back, remove the seat back cover (A).
12. | Installation is the reverse of removal.
• | To prevent wrinkles, make sure the material is stretched evenly over the cover (B) before securing the hogring clips (A).
• | Replace the hogring clips with new ones using special tool [C (09880-4F000)].
Seat Cushion Cover Replacement
1. | Remove the seat back cushion cover.
2. | Pull out the hogring clips on the front of seat cushion, remove the seat cushion cover (A).
3. | Installation is the reverse of removal.
• | To prevent wrinkles, make sure the material is stretched evenly over the cover (B) before securing the hogring clips (A).
• | Replace the hogring clips with new ones using special tool [C (09880-4F000)].
Seat Back Cover Replacement [LH]
1. | Push the lock pin (B), and then remove then headrest (A).
2. | Using a screwdriver or remover, remove the tether anchor garnish (A).
3. | zip off the seat back cover (A), and then full it up.
4. | Remove the hogring clips (A).
5. | Disonnect the hook (B).
6. | Pull out the headrest guides (A) while pinching the end of the guides, and remove them.
7. | Disconnect the seat back cover from the seat back frame.
8. | Disconnect the hogring clips (B) on the front of seat back, remove the seat back cover (A).
9. | Installation is the reverse of removal.
• | To prevent wrinkles, make sure the material is stretched evenly over the cover (B) before securing the hogring clips (A).
• | Replace the hogring clips with new ones using special tool [C (09880-4F000)].