| TUCSON(LM) >2011 > G 2.4 DOHC > Body Electrical System > Seat Electrical > Seat Heater Switch>Repair procedures |

Inspection
Front Seat Heater Switch
1. | Disconnect the negative (-) battery terminal.
2. | Remove the floor console upper cover (A) using the appropriate tool.
3. | Remove the seat heater switch module (A).
Take care not to damage the hook when removing the switch.
4. | Disconnect the driver and assist seat heater switch connector (A).
5. | Check that continuity exists between the terminals after turning the driver seat heater switch ON.
6. | Check that continuity exists between the terminals after turning the assist seat heater switch ON.
7. | If the switch fails to operate, replace the driver and assist seat heater switch (A).