| TUCSON(LM) >2011 > G 2.4 DOHC > Heating,Ventilation, Air Conditioning > Air Conditioning System > Condenser>Repair procedures |

Inspection
1. | Check the condenser fins for clogging and damage. If clogged, clean them with water, and blow them with compressed air. If bent, gently bend them using a screwdriver or pliers.
2. | Check the condenser connections for leakage, and repair or replace it, if required.
Replacement
1. | Recover the refrigerant with a recovery/ recycling/ charging station .
2. | Disconnect the negative (-) battery terminal.
3. | Remove the front bumper. (Refer to BD group - Front Bumper)
4. | Remove the discharge line and liquid line (A) from the condenser and then disconnect the condenser side cover (B).
5. | Remove the condenser (A) from radiator.
6. | Install in the reverse order of removal, and note these items :
A. | If you're installing a new condenser, add refrigerant oil ND-OIL8.
B. | Replace the O-rings with new ones at each fitting, and apply a thin coat of refrigerant oil before installing them. Be sure to use the right O-rings for R-134a to avoid leakage.
C. | Be careful not to damage the radiator and condenser fins when installing the condenser.
D. | Be sure to install the lower mount cushions of condenser securely into the holes.
E. | Charge the system, and test its performance.