| TUCSON(LM) >2011 > G 2.4 DOHC > Brake System > ESC(Electronic Stability Control) System>Schematic Diagrams |

Circuit Diagram - ESC(1)
Circuit Diagram - ESC(2)
Circuit Diagram - ESC(3)
ESC connector input/output
Connector Terminal | Specification | Remark
No | Description
29 | IGNITION1(+) | High level of wake up voltage : 4.5V < V < 16.0V Low level of wake up voltage : V < 2.4V Max. current : I < 50mA |
25 | POS. BATTERY 1.(SOLENOID) | Over voltage range : 17.0 ± 0.5V Operating voltage range : 10.0 ± 0.5V < V < 16.0 ± 0.5V Low voltage range : 7.0 ± 0.5V < V < 9.5 ± 0.5V Max. current : I < 40A Max. leakage current : I < 0.25mA |
1 | POS. BATTERY 2.(MOTOR) | Operating voltage range: 10.0 ± 0.5V < V < 16.0 ± 0.5V Rush current : I < 110A Max current : I < 40A Max leakage current : I < 0.25mA |
38 | GROUND | Rated current : I <550mA Max. current: I < 40A |
13 | PUMP MOTOR GROUND | Rush current : I < 110A Max current : I < 40A |
11 | SENSOR GROUND | Rated current : I <250mA |
4 | SENSOR POWER | Max current Capability : I < 250mA Max voltage : V_BAT1 -0.8V |
23 | BRAKE LIGHT SWITCH | Input voltage (Low) : V < 2V Input voltage (High) : V > 6V Max. Input current : I < 3mA |
9 | BRAKE SWITCH
22 | PARKING BRAKE SWITCH | Input voltage (Low) : V < 2V Input voltage (High) : V > 6V Max input current : I < 5mA |
35 | CLUTCH SWITCH (M/T Only) |
28 | SENSOR FRONT RIGHT OUTPUT | External pull up resistance :1 KΩ < R Output duty :50 ± 20% |
17 | SENSOR REAT RIGHT OUTPUT |
10 | ESC ON/OFF SWITCH | Input voltage (Low) : V < 2V Input voltage (High) : V > 6V Max input current:I <3mA |
37 | DBC SWITCH |
14 | CAN BUS LINE(LOW) | Max. Input current : I < 10mA |
26 | CAN BUS LINE(HIGH)
18 | SENSOR FRONT LEFT POWER | Output voltage : V_BAT1 -0.6v ~ V_BAT1 -1.1V Output current : Max 30mA |
34 | SENSOR FRONT RIGHT POWER
19 | SENSOR REAR LEFT POWER
33 | SENSOR REAR RIGHT POWER
31 | SENSOR FRONT LEFT SIGNAL | Input current LOW : 5.9 ~ 8.4mA Input current HIGH :11.8 ~ 16.8mA Frequency range :1 ~ 2500Hz Input duty : 50 ± 20% | Typ. 7mA Typ. 14mA
21 | SENSOR FRONT RIGHT SIGNAL
32 | SENSOR REAR LEFT SIGNAL
20 | SENSOR REAR RIGHT SIGNAL
12 | CAN SENSOR LINE (HIGH) | Max. input current : I < 10mA |
24 | CAN SENSOR LINE (LOW) |