| TUCSON(LM) >2011 > G 2.4 DOHC > Body Electrical System > Audio > Antenna>Repair procedures |

Inspection
Antenna Cable
1. | Remove the antenna jack from the audio unit and antenna.
2. | Check for continuity between the center poles of antenna cable.
3. | Check for continuity between the outer poles of antenna cable. There should be continuity.
4. | If there is no continuity, replace the antenna cable.
5. | Check for continuity between the center pole (A) and outer pole (B) of antenna cable. There should be no continuity.
6. | If there is continuity, replace the antenna cable.
Removal
1. | Remove the rear roof trim. (Refer to the BD group - "Roof trim")
2. | Disconnect the roof antenna feeder cable and connector (A) from the roof antenna.
3. | Disconnect the antenna power cable (A).
4. | Remove the roof antenna (A) after removing a nut.
Installation
1. | Connect the roof antenna cables and connectors.
2. | Install the rear roof trim.
- | Make sure that the cables and connectors are plugged in properly.
- | Check the audio system.