| TUCSON(LM) >2011 > G 2.4 DOHC > Body Electrical System > Rear Wiper/Washer > Rear Wiper Motor>Repair procedures |

Inspection
Rear Wiper Motor
1. | Remove the 4P connector from the rear wiper motor.
2. | Connect battery positive (+) and negative (-) cables to terminals 2 and 1 respectively.
3. | Check that the motor operates normally. Replace the motor if it operates abnormally.
No | Description | No | Description
1 | GND | 3 | Parking
2 | Switch | 4 | IGN(+)
Automatic Stop Operation Check
1. | Operate the motor at low speed using the stalk control.
2. | Stop the motor operation anywhere except at the off position by disconnecting terminal 2.
3. | Connect terminals 2 and 3.
4. | Connect the positive (+) lead from the battery to terminal 4 and the negative (-) lead to terminal 1.
5. | Check that the motor stops running at the off position.
Removal
1. | Detach the rear wiper head cap (A).
2. | Remove the rear wiper arm & blade (A) after removing rear wiper arm nut (B).
3. | Remove the rear wiper cover (A) and HEX nut (B).
4. | Remove the pad cap (A).
5. | Open the tailgate then remove the tailgate trim. (Refer to the BD group - "Tailgate")
6. | Disconnect the rear wiper motor connector (A) then remove the rear wiper motor (B) after loosening bolts (2EA).
Installation
1. | Install the rear wiper motor assembly.
Tightening torque Nut : 7~10 Nm (0.7~1.0 kgf.m, 5~7.4 lbf.ft)
Do not reuse the rubber pad if it is dameged.
2. | Install the tailgate trim. (Refer to the BD group - "Tailgate")
3. | Insert the pad cap and HEX nut.
Tightening torque : 4~7 Nm (0.4~0.7 kgf.m, 2.9~5.0 lbf.ft)
4. | Install the rear wiper arm and blade to align with black lowest rear defogger line (A).
5. | Install the rear wiper arm and rear wiper nut.
Tightening torque Nut : 14~17 Nm (1.4~1.7 kgf.m, 10~12 lbf.ft)