| TUCSON(LM) >2011 > G 2.4 DOHC > Manual Transaxle System > Manual Transaxle System>Repair procedures |

Service Adjustment Procedure
Transmission Oil Inspection And Replacement
1. | Park the vehicle on a level ground and stop the engine.
2. | Remove the oil filler plug and washer. Inspect the manual transaxle fluid condition and quantity.
3. | If the manual transaxle fluid is contaminated, drain it out by removing the oil drain plug.
4. | Tighten the new oil drain plug and fill manual transaxle fluid to a proper level.
Tightening torque : 29.4~34.3N.m (3.0~3.5kgf.m, 21.7~25.3lb-ft)
Oil type: SAE75W/85 Oil quantity: 1.8L (0.48 U.S.gal., 1.90 U.S.qt., 1.58 lmp.qt.)
5. | Retighten the oil filler plug with a new washer.
Tightening torque : 29.4~34.3N.m (3.0~3.5kgf.m, 21.7~25.3lb-ft)
Back Up Lamp Switch Inspection
1. | Disconnect the back up lamp switch connector (A).
2. | Inspect the continuity of the switch. When the shift lever is in reverse range, it should have continuity.
3. | Replace the back up lamp switch, if necessary.
Tightening torque : 29.4~34.4 N.m (3.0~3.5Kgf.m, 21.7~25.3lb-ft)