| TUCSON(LM) >2011 > G 2.4 DOHC > Automatic Transaxle System > Automatic Transaxle Control System > Output Speed Sensor>Repair procedures |

Removal
1. | Remove the battery and the battery tray. (Refer to "Charging system" in EE group.)
2. | Remove the under cover (A).
3. | Replace new gasket and the plug after drining the automatic transaxle fluid by removing the drain plug. (Refer to "Automatic transaxle system" in this group.)
4. | Remove the valve body cover (A) and eyebolt (B).
Tightening torque: (A) 9.8 ~ 11.8 N.m (1.0 ~ 1.2 kgf.m, 7.2 ~ 8.7 lb-ft) (B) 34.3 ~ 44.1 N.m (3.5 ~ 4.5 kgf.m, 25.3 ~ 32.6 lb-ft)
The gasket of the eyebolt use new one.
Remove installation bolts in the engin room first and then remove others under the vehicle.
5. | Remove the plate and the detend spring (A) after removing the bolt.
Tightening torque: 24.5 ~ 35.3 N.m (2.5 ~ 3.6 kgf.m, 18.1 ~ 26.0 lb-ft)
6. | Remove the bolt (3ea) after disconnecting the solenoid valve connector (A) and the oil temperature sensor connector (B).
Tightening torque: 9.8 ~ 11.8 N.m (1.0 ~ 1.2 kgf.m, 7.2 ~ 8.7 lb-ft)
Be careful not to damage the harness lock connector.
7. | Remove the valve body assembly (A).
Tightening torque: 9.8 ~ 11.8 N.m (1.0 ~ 1.2 kgf.m, 7.2 ~ 8.7 lb-ft)
8. | Disconnect the input & output speed sensor connector (A).
9. | Remove the input & output speed sensor (B) after removing the bolts(2ea).
Tightening torque: 9.8 ~ 11.8 N.m (1.0 ~ 1.2 kgf.m, 7.2 ~ 8.7 lb-ft)
Installation
1. | Installation is the reverse of removal.
After replacement or reinstallation procedure of the valve body assembly, must perform procedures below.
• | Continue to apply liquid gasket at application points at the valve body cover with Ø2.5mm (0.0984in.) thickness.
Liquid gasket Part name : Threebond 1281B or LOCTITE FMD-546
• | Adding automaticmatic transaxle fluid. (Refer to "automaticmatic transaxle system" in this group.)