| TUCSON(LM) >2011 > G 2.4 DOHC > Suspension System > Tires/Wheels > Wheel>Repair procedures |

Hub nut tightening sequence
Tighten the hub nuts as follows.
Tightening torque : 88.3 ~ 107.9N.m(9.0 ~ 11.0kgf.m, 65.1 ~ 79.6lb-ft)
When using an impact gun, final tightening torque should be checked using a torque wrench.
Run out inspection
1. | Jack up the vehicle.
2. | Measure the wheel Run-out by using a dial indicator as illustration below.
Run-out | Aluminum | Steel
Radial mm(in.) | Below 0.3(0.012) | Below 1.0(0.039)
Axial mm(in.) | Below 0.3(0.012) | Below 0.6(0.024)
3. | If measured value exceeds the standard value, replace the wheel.