| TUCSON(LM) >2011 > G 2.4 DOHC > Manual Transaxle System > General Information>Specifications |

Specifications
Manual transaxle type | M6GF2
Engine type | Gasoline 2.4
Gear ratio | 1st | 3.267
2nd | 1.794
3rd | 1.542
4th | 1.176
5th | 0.974
6th | 0.829
Reverse | 3.416
Final gear ratio | 5.071(1,2,R)
3.737(3,4,5,6)
T/M oil capacity | 1.8L (0.48 U.S.gal., 1.90 U.S.qt., 1.58 lmp.qt.)
Tightening Torques
Item | Nm | kgf.m | lb-ft
Concentric sleeve cylinder assembly | 11.8~14.7 | 1.2~1.5 | 8.7~10.8
Magnetic plug | 19.2~118.9 | 6.0~8.0 | 43.6~58.2
Shift control shaft folk and shaft guide | 19.6~26.5 | 2.0~2.7 | 14.5~19.5
Oil filler plug | 29.4~34.3 | 3.0~3.5 | 21.7~25.3
Idler shaft bolt | 24.5~29.4 | 2.5~3.0 | 18.1~21.7
Back up lamp switch | 29.4~34.3 | 3.0~3.5 | 21.7~25.3
Vehicle speed sensor | 7.8~9.8 | 0.8~1.0 | 5.8~7.2
Transaxle mounting bracket assembly | 59.2~78.9 | 6.0~8.0 | 43.6~58.2
Transaxle and engine mounting bolt | 42.2~53.9 | 4.3~5.5 | 31.1~39.8
Transaxle lower mounting bolt | 42.2~48.1 | 4.3~4.9 | 31.1~35.4
Lubricants
Item | Lubricant | Quantity
Transaxle input shaft spline | CASMOLY L9508 | 0.2 gr.
Concentric sleeve cylinder assembly | KLUBER 9R100 | As required
Transaxle case gasket | LOCTITE 587 | As required