| TUCSON(LM) >2012 > G 2.0 DOHC > Body Electrical System > Power Door Locks > Power Door Lock Switch>Repair procedures |

Removal
Driver Power Window Switch
1. | Disconnect the negative battery terminal.
2. | Remove the front door trim. (Refer to the BD group - "Front door")
3. | Remove the screws from power window switch (A) and connectors (B).
4. | Remove the driver power window switch (A) from front door trim.
Be careful not to damage the hook when removing the switch module.
Assist Power Window Switch
1. | Disconnect the negative battery terminal.
2. | Remove the front door trim. (Refer to the BD group - "Front door")
3. | Remove the power window switch (A) from front door trim.
4. | Remove the power window switch (A) from front door trim.
Be careful not to damage the hook when removing the switch module.
Installation
Driver Power Window Switch
1. | Install the driver door module and connectors.
2. | Install the front door trim.
Assist Power Window Switch
1. | Install the assist door module and connectors.
2. | Install the front door trim.