| TUCSON(LM) >2012 > G 2.0 DOHC > Manual Transaxle System > Manual Transaxle Control System > Manual Transaxle Shift Control>Repair procedures (M5GF1) |

Removal
1. | Remove the center console. (Refer to "Console" in BD group)
2. | Remove the snap pin (B) and the clip (A) from the select cable assembly.
3. | Remove the clip (A) from the shift cable assembly.
4. | Remove the shift lever assembly(A).
Tightening torque : 8.8~13.7N.m(0.9~1.4kgf.m, 6.5~10.1lb-ft)
5. | Remove the retainer(A) and nuts(B).
6. | Remove the select and shift cable assembly from the transaxle. (Refer to Transaxle removal)
Inspection
1. | Check the select cable for proper operation and for damage.
2. | Check the shift cable for proper operation and for damage.
3. | Check the boots for damage.
4. | Check the boots for wear abrasion sticking, restricted movement or damage.
5. | Check for the weak or damaged spring.
Installation
1. | Installation is the reverse of removal.
2. | Move the slide clip (B) of guide member (A) in the direction as shown in the illustration.
Adjust the slide clip fit into the select lever moving the slide clip in the direction (C).
3. | Install the guide member (A) of the select cable (B).
4. | Adjust the slide clip (B) to fit it into the select lever pin (A) and install the snap pin (C).
Insert the slide clip in the direction as shown in the illustration.