| TUCSON(LM) >2012 > G 2.0 DOHC > Body (Interior and Exterior) > Exterior > Body Side Moldings>Repair procedures |

Replacement
Roof Rack Replacement
• | When prying with a flat-tipped screwdriver, wrap it with protective tape, and apply protective tape around the related parts, to prevent damaged.
• | Put on gloves to protect your hands.
• | Take care not to scratch the body surface.
1. | Using a screwdriver or remover, remove the roof rack cover (A).
2. | After loosening the mounting nuts, then remove the roof rack (B).
3. | Installation is the reverse of removal.
Roof Molding Replacement
• | When prying with a flat-tipped screwdriver, wrap itwith protective tape, and apply protective tapearound the related parts, to prevent damaged.
• | Put on gloves to protect your hands.
• | Take care not to scratch the body surface.
1. | Remove the roof rack.
2. | Using a screwdriver or remover, remove the roof molding (A).
3. | Installation is the reverse of removal.
• | Replace any damage clips.
Tailgate Garnish Replacement
• | When prying with a flat-tipped screwdriver, wrap it with protective tape, and apply protective tape around the related parts, to prevent damaged.
• | Put on gloves to protect your hands.
• | Take care not to scratch the body surface.
1. | Remove the tail gate trim. (Refer to the BD group - "Tailgate")
2. | Disconnect the connector (A).
3. | After loosening the mounting nuts, then remove the tailgate garnish (A).
4. | Installation is the reverse of removal.
• | Replace any damage clips.
Rear Spoiler Replacement
• | When prying with a flat-tipped screwdriver, wrap itwith protective tape, and apply protective tapearound the related parts, to prevent damaged.
• | Put on gloves to protect your hands.
• | Take care not to scratch the body surface.
1. | Remove the tailgate trim. (Refer to the BD group - "Tailgate")
2. | After loosening the mounting nuts, then remove the rear spoiler (A)
3. | Disconnect the connector (A) and washer nozzle (B).
4. | Installation is the reverse of removal.
• | Replace any damage clips
Door Side Garnish Replacement
• | When prying with a flat-tipped screwdriver, wrap itwith protective tape, and apply protective tapearound the related parts, to prevent damaged.
• | Put on gloves to protect your hands.
• | Take care not to scratch the body surface
1. | Using a screwdriver or remover, remove the front door garnish (A).
2. | Using a screwdriver or remover, remove the rear door garnish (B).
3. | Installation is the reverse of removal.
• | Replace any damage clips
Side Sill Garnish Replacement
• | When prying with a flat-tipped screwdriver, wrap itwith protective tape, and apply protective tapearound the related parts, to prevent damaged.
• | Put on gloves to protect your hands.
• | Take care not to scratch the body surface.
1. | Loosen the mounting screws.
2. | Using a screwdriver or remover, remove the side sill garnish (A).
3. | Installation is the reverse of removal.
• | Replace any damage clips