| TUCSON(LM) >2012 > G 2.0 DOHC > Body Electrical System > Windshield Deicer > Windshield Deicer Switch>Repair procedures |

Removal
1. | Disconnect the negative (-) battery terminal.
2. | Remove the right air vent. (Refer to the BD group - "Crash pad")
3. | Remove the windshield deicer switch (A).
Take care not to damage the hook when removing the windshield deicer switch.
Installation
1. | Install the windshield deicer switch.
2. | Install the right air vent.
Inspection
1. | Using an ohmmeter, inspect the continuity between the terminals after removing the switch.