| TUCSON(LM) >2012 > G 2.0 DOHC > Body Electrical System > Lighting System > Hazard Lamp Switch>Repair procedures |

Removal
1. | Disconnect the negative (-) battery terminal.
2. | Remove the hazard lamp switch assembly. (Refer to the BE group - "Audio head unit")
3. | Disconnect the hazard lamp switch connector (A).
4. | If the hazard lamp switch is not as specified, replace it carefully and take care not to damage the hook (A).
Installation
1. | Connect the hazard switch connector.
2. | Install the hazard switch assembly.
Inspection
1. | Operate the switch and check for continuity between terminals with an ohmmeter.