| TUCSON(LM) >2012 > G 2.0 DOHC > Engine Electrical System > Charging System > Alternator>Repair procedures |

Disassembly
1. | Remove the alternator cover (A) using a screw driver (B).
2. | Loosen the mounting bolts (A) and disconnect the brush holder assembly (B).
3. | Remove the slip ring guide (A).
4. | Use the SST (09373-27000) remove the pulley (A).
5. | Loosen the 4 through bolts (A).
6. | Disconnect the rotor (A) and housing (B).
7. | Reassembly is the reverse order of disassembly.
Inspection
Inspect Rotor
1. | Check that there is continuity between the slip rings (C).
2. | Check that there is no continuity between the slip rings and the rotor (B) or rotor shaft (A).
3. | If the rotor fails either continuity check, replace the alternator.
Inspect Stator
1. | Check that there is continuity between each pair of leads (A).
2. | Check that there is no continuity between each lead and the coil core.
3. | If the coil fails either continuity check, replace the alternator.