| TUCSON(LM) >2012 > G 2.0 DOHC > Body Electrical System > Multifunction switch>Specifications |

Specifications
Items | Specifications
Rated voltage | DC 12V
Operating temperature range | -22 ~ +176°F (-30°C ~ +80°C)
Rated load | Dimmer & passing switch | High : 0.2A (Relay load) Low : 0.2A (Relay load) Passing : 0.2A (Relay load)
Lighting switch | Lighting : 0.2A (Relay load)
Turn signal switch | 6.6 ± 0.5A (Lamp load)
Wiper & mist switch | Low, High : 4.5A (Motor load) Intermittent : 0.22 ± 0.05A (Relay load) Lock : Max. 28A (Motor load) Mist : 4.0A (Motor load) Washer : 4.0A (Motor load)
Front fog lamp switch | 0.2A (Relay load)
Rear wiper & washer | Wiper : 1.0A (Relay load) Washer : 4.0A (Motor load)