| TUCSON(LM) >2012 > G 2.0 DOHC > 4 Wheel Drive (4WD) System > 4WD Control System > 4WD ECU>Repair procedures |

Replacement
1. | Remove the lower panel. (Refer to "Crash Pad" in BD group)
2. | Remove the IPM.(Refer to "Fuses and Relays" in BE group)
3. | Remove the parking brake pedal.(Refer to "Parking Brake System" in BR group)
4. | Remove the 4WD ECU(C) after removing the nut (A-2ea) and the connector (B).
Tightening torque: 9.8 ~ 11.8 N.m (1.0 ~ 1.2 kgf.m, 7.2 ~ 8.7 lb-ft)