| TUCSON(LM) >2012 > G 2.0 DOHC > 4 Wheel Drive (4WD) System > Coupling Assembly > Oil hydraulic Motor(Actuator)>Repair procedures |

Inspection
If you have trouble code related to the oil hydraulic motor(actuator) (P1825, P1826, P1827, P1828), check oil hydraulic motor (actuator) according to the inspection process.
Oil Hydraulic Motor (Actuator) Inspection Procedure
Removal
1. | Remove the coupling assembly. (Refer to "coupling assembly" in 4WD group)
2. | Keep going perpendicular state after remove the coupling assembly.
• | Keep going perpendicular state during remove(install) the hydraulic motor (actuators).
3. | Remove the hydraulic motor (actuators) after loosening bolts with hex wrench.
• | Remove the hydraulic motor (actuators) after dropping residual oil as much as possible inside the coupling. (abut 5~10 sec)
Installation
1. | Before installation, wipe the surface with a clean cloth.
2. | Check the O-rings of the new hydraulic motor (actuators).
• | You have to prevent any dust from entering inside hydraulic motors (actuators) and housing.
3. | Tighten the bolts after install the hydraulic motor (actuators).
• | When installing, motor connector has to toward in the direction of outside of the Coupling.
Tightening torque: 8.8 ~ 10.8 N.m (0.9 ~ 1.1 kgf.m, 6.5 ~ 8.0 lb-ft)
• | When installing, oil can be reflux by the pressure in air breather hole.(Oil reflux weight: about 5 ~ 10ml)
• | Change direction in the direction of the arrow and lay on the floor as shown in the illustration. ※ The reflux oil will flow to the bottom.
• | You have to prevent additional backflow in according to order as shown in the illustration.
4. | Wipe the flowed oil to around the surface with a clean cloth.
5. | Measure the weight of the coupling.
Coupling assembly weight: 8.18 ~ 8.23kg (Current oil capacity 490ml)
• | If the weight of the coupling assembly is less than 8.18kg, must be replace the coupling assembly because of suspect excessive reflux.