| TUCSON(LM) >2012 > G 2.0 DOHC > Engine Mechanical System > Intake And Exhaust System > Muffler>Repair procedures |

Removal
1. | Disconnect the oxygen sensor connector (A) and then remove the front muffler (B).
Tightening torque: 39.2 ~ 58.8 N.m (4.0 ~ 6.0 kgf.m, 28.9 ~ 43.4 lb-ft)
2. | Remove the catalytic converter (A) and the center muffler (B).
Tightening torque: 39.2 ~ 58.8 N.m (4.0 ~ 6.0 kgf.m, 28.9 ~ 43.4 lb-ft)
3. | Remove the main muffler (A).
Tightening torque: 39.2 ~ 58.8 N.m (4.0 ~ 6.0 kgf.m, 28.9 ~ 43.4 lb-ft)