| TUCSON(LM) >2012 > G 2.0 DOHC > Body (Interior and Exterior) > Seat Belt > Rear Seat Belt>Repair procedures |

Replacement
Secondary Seat Belt Relacement
• | When installing the belt, make sure not to damaged the retractor.
1. | Remove the rear seat. (Refer to the BD group - "Rear Seat")
2. | Remove the rear door scuff trim. (Refer to the BD group - "Interior Trim")
3. | After loosening the mounting bolt, then remove the rear seat belt lower anchor (A).
Tightening torque : 39.2 ~ 53.9 N.m (4.0 ~ 5.5 kgf.m, 28.9 ~ 39.8 lb-ft)
4. | Remove the clips.
5. | Using a screwdriver or remover, remove the transverse trim (A).
• | When prying with a flat-up screwdriver, wrap it with protective tape, and apply protective tape around the related parts, to prevent damage.
6. | After loosening the mounting bolts, then remove the rear seat bracket (A).
7. | Disconnect the lamp (A).
8. | Disconnect the connector (B).
9. | After loosening the mounting screws, then remove the luggage side trim (C).
10. | After loosening the mounting bolt and screws, then remove the rear pillar trim (A).
11. | After loosening the mounting bolts, then remove the rear seat belt (A).
Tightening torque : 39.2 ~ 53.9 N.m (4.0 ~ 5.5 kgf.m, 28.9 ~ 39.8 lb-ft)
12. | Installation is the reverse of removal.
• | Replace ant damaged clips.
Rear Seat Belt Buckle Replacement
1. | Remove the rear seat. (Refer to the BD group - "Rear Seat")
2. | Loosen the mounting bolt and then remove the seat belt buckle (A).
Tightening torque : 39.2 ~ 53.9 N.m (4.0 ~ 5.5 kgf.m, 28.9 ~ 39.8 lb-ft)
Tightening torque : 39.2 ~ 53.9 N.m (4.0 ~ 5.5 kgf.m, 28.9 ~ 39.8 lb-ft)
3. | Installation is the reverse of removal.