| TUCSON(LM) >2012 > G 2.0 DOHC > Body Electrical System > Seat Electrical > Power Seat Motor>Repair procedures |

Inspection
Power Seat Motor
1. | Remove the front seat. (Refer to BD group - "Front seat")
2. | Disconnect the connectors for each motor.
3. | With the battery connected directly to the motor terminals, check if the motors run smoothly.
4. | Reverse the connections and check that the motor turns in reverse.
5. | If there is an abnormality, replace the motors.