| TUCSON(LM) >2012 > G 2.4 DOHC > Body (Interior and Exterior) > Interior > Roof Trim>Repair procedures |

Replacement
Sunvisor Replacement
1. | After loosening the mounting screws, then remove the sunvisor (A) and retainer (B).
2. | Installation is the reverse of removal.
Assist Handle Replacement
1. | Remove the covers (A), and remove the screws, then remove the assist handle (B).
2. | Installation is the reverse of removal.
Overhead Console Replacement
1. | After loosening the mounting screws, then remove the overhead console assembly (A).
2. | Push the lock pin (A), disconnect the connectors (B).
3. | Installation is the reverse of removal.
• | Make sure the connector is plugged in properly.
Room Lamp Replacement
1. | Using a screwdriver, remove the cover (A).
2. | After loosening the mounting screws, then remove the room lamp (B).
3. | Disconnect the connector (C).
4. | Installation is the reverse of removal.
• | Make sure the connector is plugged in properly.
Vanity Lamp Replacement
1. | Using a screwdriver, remove the vanity lamp (A).
2. | Disconnect the connector (B).
3. | Installation is the reverse of removal.
Roof Trim Assembly Replacement
• | Put on gloves to protect your hands.
• | When prying with a flat-tip screwdriver, wrap it with protective tape to prevent damage.
• | Take care not to bend or scratch the trim and panels.
1. | Remove the following items.
A. | Sunvisor.
B. | Overhead console.
C. | Room lamp.
D. | Assist handle.
2. | Disconnect the cover (A) and ECM room mirror connector (B).
3. | Disconnect the cover (A) and rain sensor connector (B).
4. | Disconnect the wiring connector (A), mounting clips. [Driver's] [Passenger's]
5. | Disconnect the antenna connector (A).
6. | Disconnect the connector (B).
7. | Disconnect the clips and then remove the roof trim (A).
8. | Installation is the reverse of removal.
• | Replace any damage clips.