| TUCSON(LM) >2012 > G 2.4 DOHC > Fuel System > Engine Control System > Engine Coolant Temperature Sensor (ECTS)>Repair procedures |

Inspection
1. | Turn the ignition switch OFF.
2. | Disconnect the ECTS connector.
3. | Remove the ECTS.
4. | After immersing the thermistor of the sensor into engine coolant, measure resistance between the ECTS terminals 3 and 4.
5. | Check that the resistance is within the specification.
Specification: Refer to “Specification”
Removal
1. | Turn the ignition switch OFF and disconnect the battery negative (-) cable.
2. | Disconnect the engine coolant temperature sensor connector (A).
3. | Remove the fixing clip (A), and then pull the sensor from the water temperature control assembly.
Note that engine coolant may be flowed out from the water temperature control assembly when removing the sensor.
4. | Supplement the engine coolant (Refer to “Cooling System” in EM group).
Installation
• | Install the component with the specified torques.
• | Note that internal damage may occur when the component is dropped.
• | Apply the engine coolant to the O-ring.
• | Insert the sensor in the installation hole and be careful not to damage.
1. | Installation is reverse of removal.