| TUCSON(LM) >2012 > G 2.4 DOHC > Suspension System > Rear Suspension System > Rear Upper Arm>Repair procedures |

Replacement
1. | Remove the rear wheel & tire.
Tightening torque : 88.3 ~ 107.9N.m(9.0 ~ 11.0Kgf.m, 65.1 ~ 79.6lb-ft)
Be careful not to damage to the hub bolts when removing the front wheel & tire.
2. | Loosen the bolt & nut and then remove the rear upper arm(A) with the rear axle.
Tightening torque : 2WD 137.3 ~ 156.9N.m(14.0 ~ 16.0Kgf.m, 101.3 ~ 115.7lb-ft) 4WD 98.1 ~ 117.7N.m(10.0 ~ 12.0Kgf.m, 72.3 ~ 86.8lb-ft)
[2WD] [4WD]
3. | Loosen the bolt & nut and then remove the rear upper arm(A) with the sub frame.
Tightening torque : 2WD 137.3 ~ 156.9N.m(14.0 ~ 16.0Kgf.m, 101.3 ~ 115.7lb-ft) 4WD 98.1 ~ 117.7N.m(10.0 ~ 12.0Kgf.m, 72.3 ~ 86.8lb-ft)
[2WD] [4WD]
4. | Installation is the reverse of removal.
Inspection
1. | Check the bushing for wear and deterioration.
2. | Check the rear upper arm or damage and deformation.
3. | Check for all bolts and nut.